AMPS C/C++ Client Class Reference AMPS C/C++ Client Version 5.3.5.7

Public Member Functions | List of all members
AMPS::CompositeMessageParser Class Reference

Used to retrieve individual message parts from AMPS composite messages, which are messages where the data contains a number of parts and each part is a complete message of a specific message type. More...

`#include <CompositeMessageParser.hpp>`

## Public Member Functions
| CompositeMessageParser (void)=default
| Creates a new CompositeMessageParser with 0 valid parts.
template<class T >
size_t | parse (const T &message_)
| Parses a composite message, first clearing any existing data in the parser. More...
size_t | parse (const char *data_, size_t length_)
| Parses a composite message body, first clearing any existing data in the parser. More...
size_t | size (void) const
| Returns the number of valid message parts in the message that was last parsed.
AMPS::Field | getPart (size_t index_) const
| Returns the data of a message part. More...

## Detailed Description

Used to retrieve individual message parts from AMPS composite messages, which are messages where the data contains a number of parts and each part is a complete message of a specific message type.

For example, a composite message type of "composite-json-binary" may be declared on the server that combines a set of JSON headers with an opaque binary payload. CompositeMessageParser makes it easy to retrieve the parts of a composite message from the composite message payload. CompositeMessageParser does not make a copy of the underlying data parsed: your application must ensure that the underlying data is valid while using the CompositeMessageParser.

## Member Function Documentation

## ◆ getPart()

AMPS::Field AMPS::CompositeMessageParser::getPart | ( | size_t | index_ | ) | const
| inline

Returns the data of a message part.

Parameters

  index_ | The index of the part to retrieve.

Returns
  A Message::Field that points to the requested message part's data. If index_ is invalid, a 0-length Message::Field pointing to NULL.

## ◆ parse() [1/2]

size_t AMPS::CompositeMessageParser::parse | ( | const char * | data_,
|  | size_t | length_
| ) |  |
| inline

Parses a composite message body, first clearing any existing data in the parser.

Parameters

  data_ | A pointer to the composite message data.
  length_ | The length, in bytes, of the composite message data at data_.

Returns
  The number of valid composite message parts found in message_.

## ◆ parse() [2/2]

template<class T >

size_t AMPS::CompositeMessageParser::parse | ( | const T & | message_ | ) |
| inline

Parses a composite message, first clearing any existing data in the parser.

This function is designed to accept an AMPS::Message whose data is a composite message. It will also work for any other class that implements a getDataRaw(char**, size_t*) that sets the provided char* to the start of the payload and the provided size_t to the length of the data.

Parameters

  message_ | The AMPS::Message whose data is a composite message.

Returns
  The number of valid composite message parts found in message_.

The documentation for this class was generated from the following file:

- include/amps/CompositeMessageParser.hpp